Quality Clause 243900 - Health, Safety & Environmental Requirements (07/01/2025 - Rev A)

1) Suppliers, contractors, and sales personnel are required to wear ANSI-approved

eye protection and footwear (safety glasses and safety shoes). This condition

applies only to areas considered manufacturing and other designated areas.

2) All hazardous substances and materials delivered to or used at Bird Johnson Propeller Company facilities shall be appropriately labeled. Labels shall be undamaged, easily

readable and firmly affixed to the material and/or shipping container. Labels

shall indicate the material hazard level using the Globally Harmonized System

(GHS) as represented in the associated Safety Data Sheet (SDS).

3) Safety Data Sheets (SDS’s) shall be emailed to BirdJohnsonCerts@fmdefense.com with

the email subject line as follows: “SDS for (*insert chemical name*) on PO

XXXXXXXXXX”.

4) This must be done prior to delivery or use of a chemical or material at Bird-Johnson Propeller Company facilities. The chemical name, manufacturer, and part number shall be

referenced in the email subject line. The SDS shall accompany all chemicals and

materials delivered to or used at Bird Johnson Propeller Company facilities.

5) The SDS shall provide, at a minimum, detailed information for the chemical or

material regarding the physical properties, health hazards, exposure limits,

exposure symptoms, spill handling procedures, first aid, health effects,

toxicological data, and all other elements required under the GHS program.

6) Any vendor who supplies chemicals to perform services or other disciplines shall

remove unused chemicals from the site, including empty containers, in accordance

with all associated transportation and environmental, health, and safety

regulations.